PHP: printer_select_brush - Manual

downloads | documentation | faq | getting help | mailing lists | reporting bugs | php.net sites | links | conferences | my php.net

search for in the

printer_select_font printer_open

Last updated: Sat, 27 Jan 2007

view this page in

# printer_select_brush

(PECL)

printer_select_brush -- Select a brush

## Description

void printer_select_brush ( resource printer_handle, resource brush_handle )

The function selects a brush as the active drawing object of the actual device context. A brush is used to fill shapes. If you draw an rectangle the brush is used to draw the shapes, while the pen is used to draw the border. If you haven't selected a brush before drawing shapes, the shape won't be filled. `printer_handle` must be a valid handle to a printer. `brush_handle` must be a valid handle to a brush.

Пример 1. printer_select_brush() example

`<?php
$handle = printer_open();
printer_start_doc($handle, "My Document");
printer_start_page($handle);
$pen = printer_create_pen(PRINTER_PEN_SOLID, 2, "000000");
printer_select_pen($handle, $pen);
$brush = printer_create_brush(PRINTER_BRUSH_CUSTOM, "c:\\brush.bmp");
printer_select_brush($handle, $brush);
printer_draw_rectangle($handle, 1, 1, 500, 500);
printer_delete_brush($brush);
$brush = printer_create_brush(PRINTER_BRUSH_SOLID, "000000");
printer_select_brush($handle, $brush);
printer_draw_rectangle($handle, 1, 501, 500, 1001);
printer_delete_brush($brush);
printer_delete_pen($pen);
printer_end_page($handle);
printer_end_doc($handle);
printer_close($handle);
?>`

add a note User Contributed Notes
printer_select_brush
There are no user contributed notes for this page.
printer_select_font printer_open

Last updated: Sat, 27 Jan 2007
show source | credits | stats | sitemap | contact | advertising | mirror sites
Copyright © 2001-2007 The PHP Group
All rights reserved.
This mirror generously provided by: Yahoo! Inc.
Last updated: Sat Mar 10 10:36:09 2007 PST